Canon EOS 6D Mark II 26.2MP Digital SLR Camera with Canon EF24-105 mm f/4L is II USM Lens and Sigma 35mm F/1.4 DG HSM Art Lens

₹2,32,540.00

* Product 1: Sensor: Full frame CMOS Sensor with 26.2 MP (brilliant resolution for large prints and image cropping)
* Product 1: ISO: 100-40000 sensitivity range (critical for obtaining grain-free pictures, especially in low light)
* Product 1: Image Processor: DIGIC 7 with 45 autofocus points (important for speed and accuracy of autofocus and burst photography)
* Product 1: Video Resolution: Full HD video with fully manual control and selectable frame rates (great for precision and high-quality video work)
* Product 2: High speed with large aperture
* Product 2: Hsm (hypersonic motor) and inner focusing system
* Product 2: Accessories include: lens hood (lh730-03), carrying case
* Product 2: 35 Mm focal length, lens not zoomable

|  |  |
| --- | --- |
| Brand | ‎Canon |
| Manufacturer | ‎Canon, 1860-180-3366 |
| Model | ‎EOS 6D Mark II |
| Model Year | ‎2017 |
| Batteries | ‎1 Lithium ion batteries required. (included) |
| Item model number | ‎EOS 6D Mark II |
| Flash | ‎EF24-105mm Lens, Strap,Eyecup, Battery Charger, Battery Pack, AC Cable |
| Hardware Interface | ‎Secure Digital Card |
| Resolution | ‎26.2 |
| Special Features | ‎E-TTL II Auto Flash, Metered Manual |
| Mounting Hardware | ‎EOS 6D Body, EF24-105mm f/4L IS II USM, Battery Pack, Battery Charger, Lens Cap, Eye Cup |
| Display Technology | ‎Fully articulated LCD |
| Standing screen display size | ‎3 Inches |
| Display Type | ‎LCD |
| Image Stabilization | ‎Optical |
| Optical Zoom | ‎4 x |
| Max Resolution | ‎26.2 MP |
| Optical Sensor Resolution | ‎26.2 MP |
| Max Vertical Resolution | ‎4000 Pixels |
| Max Shutter Speed | ‎1/4000 |
| Min Shutter Speed | ‎1/30 |
| Min Focal Length | ‎24 Millimeters |
| Video Capture Resolution | ‎1080p |
| Voltage | ‎7.2 Volts |
| Batteries Included | ‎Yes |
| Batteries Required | ‎Yes |
| Battery Cell Composition | ‎Lithium Ion |
| Continuous Shooting Speed | ‎6.5 fps |
| Connector Type | ‎Wi-Fi, NFC |
| Device interface - primary | ‎Touchscreen |
| Form Factor | ‎DSLR |
| Flash Modes Description | ‎Automatic |
| Lens Type | ‎Zoom |
| Viewfinder Type | ‎Optical |
| Has Auto Focus | ‎Yes |
| Includes Rechargable Battery | ‎Yes |
| Has Self Timer | ‎Yes |
| Manufacturer | ‎Canon |

Canon Full Frame Mirrorless EOS R5 Mirrorless Camera Body  (Black)

₹3,39,995

With this Canon camera, you can kickstart your photography journey. Its 45 MP full-frame CMOS sensor will help you take detailed photos and videos. This camera can detect your subject’s body, face, or eyes and also ensures that it maintains high precision focus and tracking. You can also enjoy high-speed continuous shooting with this camera. With this camera, you can bring your creativity to life.

|  |  |
| --- | --- |
| Brand | * Canon |
| Model Number | * EOS R5 |
| Series | * Full Frame Mirrorless |
| Model Name | * Digital Camera EOS R5 |
| SLR Variant | * Body |
| Brand Color | * Black |
| Type | * Mirrorless |
| Color | * Black |
| Effective Pixels | * 45 MP |
| Tripod Socket | * Yes |
| Wifi | * Yes |
| GPS | * No |
| Face Detection | * Yes |
| Temperature | * 0 - 40 |
| Image Processor | * DIGIC X |
| Ports | * USB Type-C, HDMI Micro Out Terminal Type D, Microphone and Headphone Jack, Remote Control Terminal |
| Accessory Shoe | * Hot Shoe |
| ensor Type | * CMOS |
| Image Sensor Size | * 36 x 24 |
| ISO Rating | * Stills: 100-51 200 (L:50, H:102 400), Movie: 100-25 600 (H:51,200), RAW & HDR PQ Movies: 100-25 600, Canon Log Movies: ISO 400-25 600 (H:51 200) |
| View Finder | * Yes |
| Viewfinder Coverage | * 100% |
| Viewfinder Magnification | * Magnification/Angle of View: Approx. 0.76x/Approx. 35.5 Degree |
| Viewpoint Dioptric Adjustment | * Approx. -4.0 to +2.0 m-1 (dpt) |
| Viewfinder Eye Point | * 23 mm |
| AE Lock/Exposure Lock | * Auto: AE Lock Takes Effect When Focus is Achieved, Manual: By AE Lock Button in P, AV, FV, TV and M Modes |
| Exposure Compensation | * ±3 Stops in 1/3-stop or 1/2-stop Increments |
| Manual Exposure | * Yes |
| Shutter Speed | * 1/8000 - 30 sec |
| Shutter Steps | * Mechanical Shutter and Electronic 1st Curtain: 12, Electronic Shutter: 20 |
| Self-timer | * Yes |
| Image Stablizer | * Upto 8 Stops |
| Continuous Shots | * Upto 20 FPS |
| Shutter Type | * Electronically Controlled Focal-plane Shutter |
| Built-in Flash | * No |
| External Flash | * Yes |
| Image Format | * JPEG, HEIF, RAW, DPRAW, C-RAW |
| Aspect Ratio | * 16:9 |
| Live View Shooting | * Yes |
| HDR Support | * Yes |
| Other Image Features | * Eye, Face and Head Detection |
| Video Resolution | * 8192 x 4320 |
| Video Quality | * 8K |
| Video Format | * MP4 Video: 8K DCI/UHD (17:9/16:9) 4K DCI/UHD (17:9/16:9), Full HD |
| Display Type | * TFT Color, Liquid-crystal Monitor |
| Display Size | * 3.2 inch |
| Display Resolution | * 2100000 dots |
| Touch Screen | * Yes |
| Batteries Included | * Yes |
| Width | * 138.5 mm |
| Height | * 97.5 mm |
| Depth | * 88 mm |
| Weight | * 650 g |

# Canon EOS M6 Mark II 32.5MP + EF-M 15-45mm f/3.5-6.3 is STM Lens

₹75,250.00

* 32.5megapixel APS-C CMOS Sensor + DIGIC 8
* Dual pixel CMOS AF
* 30fps RAW burst mode (One -Shot & Servo AF)
* 5 481 selectable focus positions
* Eye Detection AF (One-Shot & Servo AF)
* Good close focusing distance of 2.5 m
* 4K Video (Uncropped/Cropped)
* Doesn’t include memory card and carry case / camera bag

|  |  |
| --- | --- |
| Brand | ‎Canon |
| Manufacturer | ‎Canon Inc., 3-30-2, Shimomaruko, Ohta-ku, Tokyo 146-8501, Japan |
| Model | ‎3611C039-C06 |
| Model Name | ‎Digital Camera |
| Product Dimensions | ‎16.5 x 16.5 x 13.5 cm; 1.05 Kilograms |
| Batteries | ‎1 D batteries required. (included) |
| Item model number | ‎3611C039-C06 |
| Flash | ‎External |
| Special Features | ‎Eye Detection Auto Focus |
| Mounting Hardware | ‎Camera, Battery Charger, AC Cable |
| Number Of Items | ‎4 |
| Standing screen display size | ‎3 Inches |
| Display Type | ‎LCD |
| Image Stabilization | ‎Optical |
| Has Image Stabilization | ‎Yes |
| Optical Zoom | ‎3 x |
| Optical Sensor Resolution | ‎32.5 MP |
| Max Shutter Speed | ‎1/8000 Seconds |
| Min Shutter Speed | ‎30 Seconds |
| Min Focal Length | ‎15 Millimeters |
| Audio Input | ‎Microphone |
| Batteries Included | ‎Yes |
| Batteries Required | ‎Yes |
| Battery Cell Composition | ‎Lithium |
| Continuous Shooting Speed | ‎30 fps |
| Form Factor | ‎Mirrorless |
| Flash Modes Description | ‎Compatible with EX-series Speedlites |
| Lens Type | ‎Zoom |
| Mounting Type | ‎EF-M mount |
| Has Self Timer | ‎Yes |
| Manufacturer | ‎Canon Inc. |
| Item Weight | ‎1 kg 50 g |

# Canon EOS M50 24.1MP Mirrorless Camera (Black) with EF-M 15-45 is STM Lens

₹80,990.00

* Sensor: APS-C CMOS sensor with 24.1 MP (high resolution for large prints and image cropping)
* ISO: 100-25600  sensitivity range (critical for obtaining grain-free pictures, especially in low light)
* Image Processor: DIGIC 8 with 143 autofocus points (important for speed and accuracy of autofocus and burst photography)
* Video Resolution: 4K video with fully manual control and selectable frame rates (excellent for precision and high-quality video work)
* Connectivity: WiFi, NFC and Bluetooth built-in (useful for remotely controlling your camera and transferring pictures wirelessly as you shoot)
* Lens Mount: Canon EF-M mount

|  |  |
| --- | --- |
| Brand | ‎Canon |
| Manufacturer | ‎Canon, 1860-180-3366 |
| Model | ‎2680C011 |
| Model Name | ‎EOS M50 |
| Model Year | ‎2018 |
| Product Dimensions | ‎5.84 x 11.68 x 8.89 cm; 388.39 Grams |
| Batteries | ‎1 D batteries required. (included) |
| Item model number | ‎2680C011 |
| Flash Memory Type | ‎SDXC |
| Flash | ‎Internal |
| Hardware Interface | ‎AV Port |
| Resolution | ‎4k uhd (3840x2160) |
| Special Features | ‎Eye Detection Auto Focus, 4K Time Lapse |
| Mounting Hardware | ‎EF M15-45 IS STM Lens, Strap, Battery Charger, Battery Pack, AC Cable |
| Number Of Items | ‎12 |
| Display Technology | ‎Vari Angle LCD |
| Standing screen display size | ‎3 Inches |
| Display Type | ‎LCD |
| Image Aspect Ratio | ‎Unknown\_aspect\_ratio |
| Image Stabilization | ‎Optical |
| Has Image Stabilization | ‎Yes |
| Optical Zoom | ‎3 x |
| Aspect Ratio | ‎Unknown |
| Resolution | ‎1,040,000 |
| Max Resolution | ‎24 MP |
| Optical Sensor Resolution | ‎24.1 MP |
| Max Vertical Resolution | ‎4000 Pixels |
| Max Shutter Speed | ‎30 Seconds |
| Min Shutter Speed | ‎30 Seconds |
| Min Aperture | ‎6.3 |
| Min Focal Length | ‎15 Millimeters |
| Video Capture Resolution | ‎2160p |
| Batteries Included | ‎Yes |
| Batteries Required | ‎Yes |
| Battery Cell Composition | ‎Lithium Ion |
| Wireless Type | ‎802.11n, 802.11b, 802.11g |
| Continuous Shooting Speed | ‎7.4 |
| Connector Type | ‎Bluetooth, Wi-Fi, NFC |
| Device interface - primary | ‎Touchscreen |
| Form Factor | ‎Mirrorless |
| Flash Modes Description | ‎Compatible with EX-series Speedlites |
| Lens Type | ‎Zoom |
| Mounting Type | ‎Canon EF |
| Viewfinder Type | ‎Electronic |
| Has Audio Recording | ‎No |
| Has Auto Focus | ‎Yes |
| Includes Rechargable Battery | ‎No |
| Has Self Timer | ‎Yes |
| Includes External Memory | ‎No |
| Supports Bluetooth Technology | ‎Yes |
| Manufacturer | ‎Canon |
| Item Weight | ‎388 g |

# Canon EOS 5D Mark 3 22.3MP Digital SLR Camera (Black) with Body Only

₹1,90,990.00

* EOS 5D Mark III is generated by a full-frame 22.3-megapixel CMOS sensor that can shoot up to 6 frames per second (fps)
* Powered by Canon's state-of-the-art DIGIC 5+ image processor; A newly expanded 61-point Auto-Focus (AF) system makes it easier to track subjects with higher levels of precision and speeds
* EOS 5D MARK III is capable of incredible ISO speeds of up to 25600 (expandable to 102400)
* Wide, 3.2-inch TFT colour, liquid crystal monitor with Approx. 1.04 million dots; Viewfinder: Eye-level pentaprism with Approx. -3.0 - +1.0 m-1 (dpt) built-in Dioptric Adjustment
* EOS HD video with manual exposure control and multiple frame rates (1080: 30p (29.97) / 24p (23.976) / 25p, 720: 60p (59.94) / 50p, 480: 30p (29.97) / 25p) with 4 GB automatic file partitioning (continuous recording time 29 minutes 59 seconds), selectable All i-frame or IPB compressions, embedded timecode, manual audio level control while recording and headphone terminal
* Eye Cap, EOS Digital solution Disk, Stereo AV cable AVC-DC400ST, Battery pack LP-E6, Battery charger LC-E6 or LC-E6E, Interface cable IFC-200U, Wide strap EW-EOS5DMKIII, Software instruction manual
* 2 Years Warranty

|  |  |
| --- | --- |
| Brand | ‎Canon |
| Manufacturer | ‎Canon |
| Model | ‎5260B021 |
| Model Name | ‎EOS Digital |
| Model Year | ‎2012 |
| Product Dimensions | ‎15.2 x 7.64 x 11.64 cm; 950 Grams |
| Item model number | ‎5260B021 |
| Hardware Interface | ‎PictBridge |
| Resolution | ‎21.1 megapixels |
| Mounting Hardware | ‎EOS 5D Mark III Digital SLR Body, Battery Pack LP-E6, Battery Charger LC-E6, Wide Neck Strap EW-EOS5DMKIII, USB Interface Cable IFC-200U, Stereo Video Cable AVC-DC400ST, Eyecup Eg, EOS Digital Solution Disk, Software Instruction Manual CD, Camera Basic instruction Manual Booklet, CF Card |
| Standing screen display size | ‎3.2 Inches |
| Display Type | ‎TFT colour, liquid-crystal monitor |
| Has Image Stabilization | ‎No |
| Optical Zoom | ‎40 |
| Digital Zoom | ‎4 x |
| Aspect Ratio | ‎1.55:1 |
| Max Resolution | ‎23.4 MP |
| Optical Sensor Resolution | ‎21.1 MP |
| Max Vertical Resolution | ‎3840 Pixels |
| Max Shutter Speed | ‎30 Seconds |
| Min Focal Length | ‎24 Millimeters |
| Batteries Included | ‎No |
| Batteries Required | ‎Yes |
| Form Factor | ‎DSLR |
| Viewfinder Type | ‎Optical |
| Has Auto Focus | ‎Yes |
| Includes Rechargable Battery | ‎No |
| Has Self Timer | ‎Yes |
| Includes AC Adapter | ‎No |
| Remote Control Included? | ‎No |
| Includes External Memory | ‎No |
| Manufacturer | ‎Canon |
| Item Weight | ‎950 g |

# Canon EOS 90D Digital SLR Camera with 18-135 is USM Lens

₹1,24,990.00

* High image quality with 32.5 Megapixel CMOS (APS-C) sensor
* High-speed continuous shooting of up to 10 fps
* 4K UHD 30P/ Full HD 120P video
* 45-Point All Cross-type AF System\* supports up to 27 points with an F/8 metering
* Equipped with an approx. 220, 000 Pixel new AE sensor and EOS iTR AF (face detection)
* Country of Origin: Japan

|  |  |
| --- | --- |
| Brand | ‎Canon |
| Manufacturer | ‎Canon Inc., 3-30-2, Shimomaruko, Ohta-ku, Tokyo 146-8501, Japan |
| Model | ‎EOS 90D 18-135 IS USM |
| Model Name | ‎Canon EOS |
| Model Year | ‎2019 |
| Product Dimensions | ‎28 x 22 x 16 cm; 1.96 Kilograms |
| Batteries | ‎1 Lithium ion batteries required. (included) |
| Item model number | ‎EOS 90D 18-135 IS USM |
| Flash | ‎Internal |
| Hardware Interface | ‎Secure Digital Card |
| Resolution | ‎32.5 |
| Special Features | ‎Eye Detection Auto Focus |
| Mounting Hardware | ‎Camera, Battery Charger, AC Cable |
| Number Of Items | ‎1 |
| Display Technology | ‎Fully articulated LCD |
| Standing screen display size | ‎3 Inches |
| Image Stabilization | ‎Optical |
| Has Image Stabilization | ‎Yes |
| Optical Zoom | ‎7.5 x |
| Aspect Ratio | ‎1.50:1 |
| Max Resolution | ‎32.5 MP |
| Optical Sensor Resolution | ‎32.5 MP |
| Max Shutter Speed | ‎1/8000 Seconds |
| Min Shutter Speed | ‎30 Seconds |
| Min Focal Length | ‎18 Millimeters |
| Video Capture Resolution | ‎2160p |
| Voltage | ‎230 Volts |
| Batteries Included | ‎Yes |
| Batteries Required | ‎Yes |
| Battery Cell Composition | ‎Lithium Ion |
| Continuous Shooting Speed | ‎10 fps |
| Connector Type | ‎Wi-Fi |
| Material | ‎Polycarbonate resin |
| Form Factor | ‎DSLR |
| Flash Modes Description | ‎Compatible with EX-series Speedlites |
| Lens Type | ‎Zoom |
| Mounting Type | ‎Canon EF-S |
| Viewfinder Type | ‎Optical |
| Includes Rechargable Battery | ‎Yes |
| Has Self Timer | ‎Yes |
| Includes AC Adapter | ‎Yes |
| Manufacturer | ‎Canon Inc. |
| Country of Origin | ‎Japan |
| Imported By | ‎3-30-2, Shimomaruko, Ohta-ku, Tokyo 146-8501, Japan |
| Item Weight | ‎1 kg 960 g |

# Canon PowerShot SX430 IS 20MP Digital Camera with 45x Optical Zoom (Black)

₹18,950.00

* 45x optical zoom (24 - 1080mm) with 90x ZoomPlus
* 20.0 megapixels sensor
* Intelligent IS
* Wi-Fi and NFC

|  |  |
| --- | --- |
| Brand | ‎Canon |
| Manufacturer | ‎Canon Inc., Canon Inc. |
| Model | ‎SX430B |
| Model Name | ‎PowerShot |
| Product Dimensions | ‎16 x 14.5 x 10.5 cm; 600 Grams |
| Batteries | ‎1 D batteries required. |
| Item model number | ‎SX430B |
| Resolution | ‎20 megapixels |
| Special Features | ‎Time-lapse |
| Mounting Hardware | ‎Camera, Battery Charger, AC Cable |
| Number Of Items | ‎1 |
| Display Technology | ‎LCD |
| Display Type | ‎LCD |
| Image Stabilization | ‎Optical |
| Optical Zoom | ‎45 x |
| Resolution | ‎720p HD Ready |
| Optical Sensor Resolution | ‎20 MP |
| Max Shutter Speed | ‎1/4000 Seconds |
| Min Focal Length | ‎24 Millimeters |
| Video Capture Resolution | ‎1080p |
| Batteries Included | ‎No |
| Batteries Required | ‎Yes |
| Battery Cell Composition | ‎Lithium Ion |
| Connector Type | ‎Wi-Fi |
| Lens Type | ‎Zoom |
| Manufacturer | ‎Canon Inc. |
| Country of Origin | ‎China |
| Imported By | ‎Xingchuang 2nd Rd, Binhu District, Wuxi, Jiangsu, China |
| Item Weight | ‎600 g |

# Canon EOS R Mirrorless Digital Camera with 24-105mm Lens

2,49,990.00

* 30.3MP full-frame CMOS sensor DIGIC 8 image processor UHD 4K30 video, C-log and 10-Bit HDMI out dual pixel CMOS AF, 5655 AF points
* Two years Canon India warranty card included
* 30.3MP full-frame CMOS sensor and DIGIC 8 image processor
* Dual pixel CMOS AF
* UHD 4K video recording and Canon log gamma

|  |  |
| --- | --- |
| Brand | ‎Canon |
| Manufacturer | ‎Canon Inc |
| Model | ‎3075C012 |
| Model Name | ‎Canon EOS |
| Model Year | ‎2018 |
| Product Dimensions | ‎8.38 x 13.46 x 9.91 cm; 1.4 Kilograms |
| Batteries | ‎1 Lithium ion batteries required. (included) |
| Item model number | ‎3075C012 |
| Hardware Interface | ‎AV Port |
| Special Features | ‎Time-lapse |
| Mounting Hardware | ‎Camera, Lens, Battery, Battery Charger |
| Number Of Items | ‎2 |
| Standing screen display size | ‎3.15 Inches |
| Display Type | ‎LCD |
| Image Stabilization | ‎Digital |
| Has Image Stabilization | ‎No |
| Optical Zoom | ‎4.3 x |
| Aspect Ratio | ‎Unknown |
| Max Resolution | ‎30.3 MP |
| Min Aperture | ‎22 |
| Min Focal Length | ‎24 Millimeters |
| Video Capture Resolution | ‎2160p |
| Batteries Included | ‎Yes |
| Batteries Required | ‎Yes |
| Battery Cell Composition | ‎Lithium Ion |
| Continuous Shooting Speed | ‎8 fps |
| Connector Type | ‎HDMI |
| Form Factor | ‎Mirrorless |
| Lens Type | ‎Wide Angle |
| Viewfinder Type | ‎Electronic |
| Includes Rechargable Battery | ‎Yes |
| Has Self Timer | ‎Yes |
| Includes External Memory | ‎No |
| Manufacturer | ‎Canon Inc |
| Item Weight | ‎1 kg 400 g |

# Canon EOS M100 24.2 Megapixels Mirrorless Camera with 13 Multiplier\_x (Black)

₹1,78,499.00

* Dual Pixel CMOS AF with Phase-detection
* It has 24.2 Megapixel CMOS (APS-C) Sensor
* Built-in Wi-Fi, NFC and Bluetooth
* Intuitive Touchscreen, 3.0-Inch Tilt-type LCD
* Built-in Wi-Fi, NFC and Bluetooth. Intuitive Touchscreen, 3.0-inch Tilt-type LCD.1 Year Manufacturer's Warranty

|  |  |
| --- | --- |
| Manufacturer | ‎Canon |
| Model | ‎2209C021 |
| Model Year | ‎2017 |
| Product Dimensions | ‎3.56 x 10.92 x 6.6 cm; 303.34 Grams |
| Batteries | ‎1 Lithium ion batteries required. (included) |
| Item model number | ‎2209C021 |
| Hardware Interface | ‎AV Port |
| Standing screen display size | ‎3 Inches |
| Display Type | ‎LCD |
| Has Image Stabilization | ‎Yes |
| Optical Zoom | ‎13 x |
| Aspect Ratio | ‎16:9 |
| Max Resolution | ‎24.2 MP |
| Optical Sensor Resolution | ‎24.2 MP |
| Max Vertical Resolution | ‎4000 Pixels |
| Min Aperture | ‎6.3 |
| Min Focal Length | ‎15 Millimeters |
| Batteries Included | ‎Yes |
| Batteries Required | ‎Yes |
| Battery Cell Composition | ‎Lithium Ion |
| Continuous Shooting Speed | ‎4 |
| Connector Type | ‎Bluetooth, Wi-Fi, NFC |
| Form Factor | ‎Mirrorless |
| Lens Type | ‎Mirror |
| Includes Rechargable Battery | ‎Yes |
| Has Self Timer | ‎Yes |
| Includes External Memory | ‎No |
| Manufacturer | ‎Canon |
| Item Weight | ‎303 g |

# Canon EOS 200D II 24.1MP Digital SLR Camera + EF-S 18-55mm f4 is STM Lens (Black)

₹51,499.00

* DIGIC 8 PROCESSOR
* APS-C Approx 24.1 mp CMOS Sensor
* 9-point AF during optica viewfinder shooting
* Dual Pixel CMOS AF
* Eye detection AF
* Doesn’t include memory card and carry case / camera bag
* 4K Movie, Closest Focusing Distance (cm): 25
* 4K time-lapse movie
* Movie Digital IS
* Country of Origin: Taiwan

|  |  |
| --- | --- |
| Brand | ‎Canon |
| Manufacturer | ‎Canon Inc., No.18, Chen Kuo Road, Tan Tzu Dist, Taichung City, Taiwan |
| Model | ‎EOS 200D II |
| Model Name | ‎EOS |
| Model Year | ‎2019 |
| Product Dimensions | ‎22 x 17 x 14 cm; 1.22 Kilograms |
| Batteries | ‎1 Lithium Metal batteries required. (included) |
| Item model number | ‎EOS 200D II |
| Memory Storage Capacity | ‎16 GB |
| Flash | ‎EF S18-45 IS II Lens, Strap, Battery Charger, Battery Pack, AC Cable |
| Hardware Interface | ‎Secure Digital Card |
| Special Features | ‎Eye Detection Auto Focus |
| Mounting Hardware | ‎EF S18-45 IS II Lens, Strap, Battery Charger, Battery Pack, AC Cable |
| Number Of Items | ‎2 |
| Display Technology | ‎Fully articulated LCD |
| Standing screen display size | ‎3 Inches |
| Display Type | ‎LCD |
| Image Stabilization | ‎Optical |
| Has Image Stabilization | ‎Yes |
| Optical Zoom | ‎3 x |
| Aspect Ratio | ‎4:3 |
| Max Resolution | ‎24.1 MP |
| Optical Sensor Resolution | ‎24.1 MP |
| Max Shutter Speed | ‎1/4000 Seconds |
| Min Shutter Speed | ‎30 Seconds |
| Min Focal Length | ‎18 Millimeters |
| Video Capture Resolution | ‎2160p |
| Voltage | ‎230 Volts |
| Batteries Included | ‎Yes |
| Batteries Required | ‎Yes |
| Battery Cell Composition | ‎Lithium Ion |
| Continuous Shooting Speed | ‎5 fps |
| Connector Type | ‎Wi-Fi |
| Device interface - primary | ‎Touchscreen, Dial, Buttons |
| Material | ‎Polycarbonate resin |
| Form Factor | ‎DSLR |
| Flash Modes Description | ‎Compatible with EX-series Speedlites |
| Lens Type | ‎Zoom |
| Mounting Type | ‎Canon EF-S |
| Viewfinder Type | ‎Optical |
| Has Auto Focus | ‎Yes |
| Includes Rechargable Battery | ‎Yes |
| Has Self Timer | ‎Yes |
| Includes AC Adapter | ‎Yes |
| Remote Control Included? | ‎No |
| Manufacturer | ‎Canon Inc. |
| Country of Origin | ‎Taiwan |
| Imported By | ‎No.18, Chen Kuo Road, Tan Tzu Dist, Taichung City, Taiwan |
| Item Weight | ‎1 kg 220 g |